|  |  |
| --- | --- |
|  | **Compress air** |
|  |  |  |  |  |
|  | Providing a drainpipe, and valve at the lowest point of every air receiver and automatic traps to prevent the accumulation oil and water. |
|  |  |  |  |  |
|  | Providing air receivers with pressure gage to prevent pressure in the receiver from exceeding the maximum allowable working pressure of the receiver by more than 10 percent. |
|  |  |  |  |  |