Hazards Associated with Non-Routine Tasks

Methods to be safe:

1. Upon initial hire, employees are informed that they should consult his/her Supervisor when the employees are either unaware of the hazards associated with a new task or if they lack knowledge of potential hazards in their workspace (unmarked pipes etc.)
2. Upon notification, the Supervisor shall do a hazard assessment of the task or work environment and inform the employee of the associated hazards. The employee will not commence work until the task or work environment has been assessed (where pipes are unmarked, the Supervisor shall label these pipes to avoid potential future confusion).