|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **TABLE I–4.—GLOVE TESTS—WATER LEVEL 1, 2** | | | | | | |
|  | **Class of glove** | **AC proof test** | | **DC proof test** | |  |
| **mm.** | **in.** | **mm.** | **in.** |
| 0 | 38 | 1.5 | 38 | 1.5 |
| 1 | 68 | 1.5 | 51 | 2.0 |
| 2 | 64 | 2.5 | 76 | 3.0 |
| 3 | 89 | 3.5 | 102 | 4.0 |
| 4 | 127 | 5.0 | 153 | 6.0 |
| 1The water level is given as the clearance from the cuff of the glove to the water line, with a tolerance of +13 mm. (+0.5 in.).  2If atmospheric conditions make the specified clearances impractical, the clearances may be increased by a maximum of 25 mm. (1 in.). | | | | | | |